

## Developer Technical Services

**Assignment #1**

API Overview

**Topics Covered**


* How to find API Docs
* Build a very basic plug-in: HelloWorldCmd
* Working with the structure of plug-ins: SineNode

**Assignments**

* For every Plug-in, we will provide an “Exercise” folder and a “Solution” folder. Each includes a Visual Studio solution and corresponding files. Solution folder includes the complete code for you to finish the Plug-in, it is for you to reference when you are stuck at problems when adding code into “Exercise” folder. In the “Exercise” folder, all the code you need to finish is specified with comments “//- TODO:”, you need to search for all the “TODO” comments and add your code there.

**Background**

* **How to find API Docs**
  1. On Windows XP:
     + Start Menu > Programs > Autodesk > Autodesk Maya 2009 > View Maya Documentation
  2. At the bottom of the left pane, select ‘API’. Or click on the “API Classes” links on the right upper corner under the “Quick Links” section.

****

* **Configuring Your Maya Plug-in Path**

1. Browse to the folder:

C:\My Documents\maya\2009 or

C:\My Documents\maya

2. Create a text file named: Maya.env

3. In Maya.env, insert the line:

MAYA\_PLUG\_IN\_PATH=C:\MayaAPITraining\plug-ins

* **Tips: Safely reloading a plug-in without restarting Maya**
  1. Clear the scene:
     + File > New Scene
     + file –f –new
  2. Clear the undo queue:
     + flushUndo
  3. Unload the plug-in:
     + unloadPlugin helloWorld.py
  4. Reload the plug-in:
     + loadPlugin helloWorld.py

**helloWorldCmd Plug-in**

* **Topics Covered**

Implement a simple custom python command “spHelloWorld”. It demonstrates the skeleton code implementation for a python command plug-in with MPxCommand.

* **Overview**

In this Plug-in, we will create a custom command “spHelloWorld” in python, which prints out “Hello World!” in the script editor window.

* **Exercises**

1. Go to “helloWorld python Plug-in\Exercise” folder, open helloWorldCmd.py, the skeleton of the command is already there.
2. Add corresponding code into the skeleton to make it work.

Relevant Classes and commands:

import sys

import maya.OpenMaya as OpenMaya

import maya.OpenMayaMPx as OpenMayaMPx

def \_\_init\_\_(self)

def doIt(self,argList)

OpenMayaMPx.asMPxPtr()

* **Result**

In maya script editor, python tab, execute the following line:

import maya

maya.cmds.loadPlugin("helloWorldCmd.py")

maya.cmds.spHelloWorld()

You will see “Hello World!” printed out in the script editor

**sineNode Plug-in**

* **Topics Covered**

Implement a custom python node “spSineNode”. It demonstrates the skeleton code implementation for a python node plug-in with MPxNode.

* **Overview**

In this Plug-in, we will create a custom node “spSineNode” in python, this node has an input attribute “input” and an output attribute ”output”, the “output” is a sine calculation of “input”.

* **Exercises**

1. Go to “sineNode python Plug-in\Exercise” folder, open sineNode.py, the skeleton of the node is already there.
2. Add corresponding code into the skeleton to make it work.

Relevant Classes and commands:

import sys,math

import maya.OpenMaya as OpenMaya

import maya.OpenMayaMPx as OpenMayaMPx

OpenMaya.MObject()

OpenMayaMPx.asMPxPtr()

def compute(self,plug,dataBlock)

* **Result**

In Maya, load the plug-in “sineNode.py”, execute the following script:

polySphere;

createNode spSineNode -n sine1;

connectAttr time1.outTime sine1.input;

connectAttr time1.outTime pSphere1.translateX;

connectAttr sine1.output pSphere1.translateY;

You will find a polySphere created and move along X axis as time goes on.

**Assignment #2**

Maya Nodes Part 1

**Topics Covered**

* Build Maya Custom Node with MPxNode

**simpleNode Plug-in**

* **Topics Covered**
  + Write a skeleton of a custom node “simpleNode” with MPxNode class from scratch
  + Add simple attribute using MFnNumericAttribute class
* **Overview**
  + In this exercise, we will implement a custom node simpleNode, it has two attributes: “input”, ”output”

Whenever the “input” attribute changes value, the “output” attribute will always be the “input” attribute value multiplied by 2.

* **Exercises**
  + 1.Assuming you already copied the whole Plug-in under C:\MayaAPITraining, go to C:\MayaAPITraining\simpleNode\Exercise\
  + 2. Double click on simpleNode.py to open the Plug-in, the skeleton of the simpleNode has already been provided.
  + 3. In simpleNode.py, adding declaration of “output” attributes and also declare your unique node ID
  + 4. In simpleNode.py, implement functions that are declared in simpleNode.py.

Relevant classes and methods:

MFnNumericAttribute::create()

MPxNode::attributeAffects(), MPxNode::addAttribute()

MDataBlock::outputValue(), MDataBlock::setClean()

MDataHandle::set()

* + 5. In simpleNode.py, implement both initializePlugin() and uninitializePlugin() functions to handle registration and de-registration of the simpleNode node.

Relevant classes and methods:

MFnPlugin:: registerNode()

MFnPlugin:: deregisterNode()

* **Result**

In script editor, execute:

createNode simpleNode;

Open “Attribute Editor”, you will see there are two attributes listed, “input”, “output”. If you change “input” value, “output” value will be 2\* input.

**transCircleNode Plug-in**

* **Topics Covered**
  + Write a custom node “transCircleNode” with MPxNode class
  + Add compound attribute using MFnNumericAttribute
  + Implement functions of transCircleNode to achieve the functionality so that the output attribute’s value is the value of inputTranslate plus the value of a circular movement based on current time frame.
* **Overview**
  + In this exercise, we will implement a custom node transCircleNode, it takes in two input attributes and one output:

A compound input translate attribute “inputTranslate”, composes of three elements: translateX, translateY, and translateZ

An input attribute “input”: current time

An input attribute “frames”: rotating speed (frames per circle)

An input attribute “scale”: decides the radius of the circle

An output a translate attribute “outputTranslate”, the value of outputTranslate is the value of inputTranslate plus the value of a circular movement based on current time frame.

* **Exercises**
  + 1. Double click on “transCircleNode.py” to open the Plug-in, the skeleton of the transCircleNode has already been provided.
  + 2. Implement transCircleNode.py, declare output attributes
  + 3. Implement transCircleNode.py

Relevant classes and methods:

MFnCompoundAttribute::create() MFnCompoundAttribute::addChild()

MDataBlock::inputValue(), MDataBlock::outputValue()

* + 4. Put AEtransCircleTemplate.mel to

C:\My Documents\maya\2009\prefs\scripts

* **Result:**

Open a new scene, execute the following script in Script Editor:

createNode transCircle -n circleNode1;

sphere -n sphere1 -r 1;

sphere -n sphere2 -r 2;

connectAttr sphere2.translate circleNode1.inputTranslate;

connectAttr circleNode1.outputTranslate sphere1.translate;

connectAttr time1.outTime circleNode1.input;

You will see two nurbs sphere created and once you hit the “play” button, one sphere is rotating around the bigger sphere; you can also set the radius of the circle, and rotating speed by setting the values in attribute editor of circleNode1.

**Assignment #3**

Maya Nodes Part 2

**Topics Covered**

* Dynamic attribute on MPxNode

**Assignments**

For every Plug-in, we will provide an “Exercise” folder and a “Solution” folder. Each includes a Visual Studio solution and corresponding files. Solution folder includes the complete code for you to finish the Plug-in, it is for you to reference when you are stuck at problems when adding code into “Exercise” folder. In the “Exercise” folder, all the code you need to finish is specified with comments “//- TODO:”, you need to search for all the “TODO” comments and add your code there.

**dynNode Plug-in**

* **Topics Covered**
  + Create dynamic attribute using MFnNumericAttribute and add it in MPxNode::postConstructor()
  + Set up affecting relationship between dynamic attribute and general attribute
* **Overview**
  + In this exercise, custom node “dynNode” has two attributes: “input” and “output”. We will add a dynamic attribute “dynAttr” on this class, also set up the affecting relationship so that the value of “output” is the sum of “input” and “dynAttr”.
* **Exercises**
  + 1. Double click on “dynNode.py” to open the Plug-in, the skeleton of the dynNode has already been provided.
  + 2. Implement dynNode.py, add necessary function declaration

Relevant classes and methods:

MPxNode::postConstructor()

MPxNode::setDependentDirty()

* + 3. Implement dynNode.py, create a dynamic attribute, set up affecting relationship between it and output attribute, also in compute(), set up so that output = input + dynAttr

Relevant classes and methods:

MFnNumericAttr::create()

MPxNode:: thisMObject()

MFnDependencyNode::addAttribute()

MDataBlock::inputValue()

MDataHandle::asFloat()

* **Result**

In script editor, execute:

createNode dynNode;

Open “Attribute Editor”, you will see there are three attributes listed, “input”, “output” and “dynAttr”. If you change “dynAttr” value, and refresh the attribute editor, you will see “output” value will be the value of “input” plus the value of “dynAttr”.

**Assignment #4**

Maya Commands

**Topics Covered**

* Build Maya custom command with MPxCommand
* Parse command arguments with MSyntax and MArgDatabase
* Support undo/redo of a custom command
* Use Iterator class to traverse selected objects
* Retrieve plug information with MFnDependencyNode and manipulate compound plug values
* Retrieve instancing information and matrix information with MDagPath

**nodeInfoCmd Plug-in**

* **Topics Covered**
  + Write a custom command “nodeInfoCmd” with MPxCommand class from scratch
  + Implement flag argument for MPxCommand with MSyntax class
  + Retrieve node type information and plug information with MFnDependencyNode and MPlug
* **Overview**
  + In this exercise, we will implement a custom command nodeInfoCmd, with an option to specify a flag “-quiet”. By default, for all the selected nodes in the scene, it will print out all the node types and connected plugs information and also the node which is connecting to this selected node as a source. If “-quiet” is provided by user, the command will only print out the selected node type.
* **Exercises**
  + 1. Double click on “nodeInfoCmd.py”
  + 2. Implement nodeInfoCmd.py, add necessary function declaration

Relevant classes and methods:

MPxCommand::doIt()

* + 3. Implement nodeInfoCmd.py,

Relevant classes and methods:

MSyntax::addFlag(), MArgDatabase::isFlagSet()

MGlobal::getActiveSelectionList()

MItSelectionList::getDependNode()

MFnDependencyNode::MFnDependencyNode()

MFnDependencyNode::getConnections()

MPlug::connectedTo()

* + 4. In nodeInfoCmd.py, implement both initializePlugin() and uninitializePlugin() functions to handle registration and de-registration of the nodeInfoCmd command.

Relevant classes and methods:

MFnPlugin:: registerCommand()

MFnPlugin:: deregisterCommand()

* **Result**
  + In any Maya scene, select a node that has connections and in script editor, execute: nodeInfoCmd, it will print out the node type and all the connected plugs information and also print out the node which is the source of the connection.
  + You can also create the transCircle node and set it up as in the transCircle Plug-in, select transCircle node, you will be able to print out its connected plug information.

**Assignment #5**

Dependency Graph

**retrieveWeight Plug-in**

* **Topics Covered**

Implement a custom command, which retrieves information from multi attribute “weight” of a blendShape node with class MPlug. It demonstrates how to traverse the element plugs and get value from array plug outside of a node.

* **Overview**

In this Plug-in, we will create a custom command “retrieveWeight”, it searches attribute “weight” on blendShape node and since it is a multi attribute, it prints out the number of elements in this array attribute and traverse the array to print out plug data on every element.

* **Exercises**
  + 1. Double click on retrieveWeight.py, the skeleton of the retrieveWeightCmd has already been provided.
  + 2. Implement retrieveWeightCmd.py, add necessary function declaration
  + 3. Implement retrieveWeightCmd.py, in doIt() function, get a hold of “blendShape” in the scene and find out “weight” on this node and print out all multi attribute information on this node.

Relevant classes and methods:

MFnDependencyNode::findPlug()

MPlug::isArray(), MPlug::numElements()

MPlug::elementByPhysicalIndex(), MPlug::logicalIndex()

MPlug::getValue()

* + 4. In retrieveWeightCmd.py, implement both initializePlugin() and uninitializePlugin() functions to handle registration and de-registration of the retrieveWeight command.

Relevant classes and methods:

MFnPlugin::registerCommand()

MFnPlugin::deregisterCommand()

* **Result**

Open scene file blendShape-2009.mb. Find the blendShape1 node and select it, then execute “retrieveWeight”. It will print out the array attribute name, how many elements this array has, the physical and logical index of all the elements in the array and the weight value of each target shape stored in every element of the array.

**Assignment #6**

Miscellaneous Tools

**Topics Covered**

* Manipulate Dependency Graph through MDGModifier class
* Implement scene callback functions with MSceneMessage class

**setUpTransCircle Plug-in**

* **Topics Covered**
  + Implement a custom command and use MDGModifier to manipulate Dependency Graph (such as adding nodes, building connections)
  + Support undo/redo
* **Overview**
  + In this exercise, we will create a custom command, and simulate the same functionality of the MEL operations we used in Lab 1 “transCircleNode” Plug-in, which set up the transCircle node.

Here are the commands you need to simluate:

createNode transCircle -n circleNode1;

sphere -n sphere1 -r 1;

sphere -n sphere2 -r 2;

connectAttr sphere2.translate circleNode1.inputTranslate;

connectAttr circleNode1.outputTranslate sphere1.translate;

connectAttr time1.outTime circleNode1.input;

* **Exercises**
  + 1. Double click on setUpTransCircle.py,the skeleton of the setUpTransCircle has already been provided. Note that this Plug-in also includes the source code for transCircleNode.
  + 2. Implement setUpTransCircleCmd.py, add necessary function declaration and member variable declaration.

Relevant classes and methods:

MPxCommand:: isUndoable(), MPxCommmand::undoIt(), MPxCommand::redoIt()

Since you want to support undo/redo, you may want to declare an MDGModifier object as a member variable.

* + 3. Implement setUpTransCircleCmd.py, in doIt() functions, simulate the MEL commands using your member variable MDGModifier object.

Relevant classes and methods:

MDGModifier::createNode(), MDGModifier::renameNode()

MDGModifier::commandToExecute()

MDGModifier::doIt(), MDGModifier::undoIt(),

MDGModifier::redoIt() , MDGModifier::connect()

MGlobal::getSelectionListByName()

MSelectionList::getDependNode()

MFnDependencyNode::attribute()

* + 4. In setUpTransCircleCmd.py, implement both initializePlugin() and uninitializePlugin() functions to handle registration and de-registration of the setUpTransCircle command.

Relevant classes and methods:

MFnPlugin::registerCommand()

MFnPlugin::deregisterCommand()

Note: you will also need to register “transCircle” node to make it work. Relevant classes and methods:

MFnPlugin::registerNode()

MFnPlugin::deregisterNode()

* **Result**

After you finish and load the plug-in setUpTransCircle.py, execute the follow command:

setUpTransCircle;

You will see two nurbs sphere created and once you hit the “play” button, one sphere is rotating around the bigger sphere, you can also set the radius of the circle, and rotating speed by setting the values in attribute editor of circleNode1.

* **Bonus Section**

You can use dgMod.commandToExecute() to simulate MEL command “sphere -n sphere1 -r 1;”, however you can also simulate the operations from scratch. Go into the hypergraph and try to find what have happened to the Dependency Graph (for examples, what nodes have been created and what connections have been made) when you execute “sphere -n sphere1 -r 1;” and simulate those changes with MDGModifier.

Tips: There are mainly two types of nodes created, “nurbsSurface” and “makeNurbSphere”, they are connected:

makeNurbSphere1.outputSurface🡪sphere1Shape.create

**sceneMsgCmd Plug-in**

* **Topics Covered**
  + How to use MSceneMessage to register callbacks watching scene operations
* **Overview**
  + In this exercise, we will create a custom command to watch specific scene operation messages:

MSceneMessage::kBeforeOpen,

MSceneMessage::kAfterNew,

MSceneMessage::kBeforeSaveCheck

We will implement callback functions which get trigger by those messages. We will also experiment how to abort current scene operation by using checkCallback functions.

* **Exercises**
  + 1. Go to “sceneMsgCmd\Exercise” folder, double click on sceneMsgCmd.py, the skeleton for this command is already implemented.
  + 2. Implement sceneMsgCmd.py, add necessary function declaration and member variable declaration.

Relevant classes and functions:

MPxCommand::isUndoable(), MPxCommmand::undoIt(), MPxCommand::redoIt()

To keep a list of all the registered callbacks, you may want to declare a member variable to record all the callback IDs.

* 3. Implement sceneMsgCmd.py, in redoIt() function, register callbacks for MSceneMessage::kBeforeOpen, MSceneMessage::kAfterNew, MSceneMessage::kBeforeSaveCheck

Relevant classes and functions:

MSceneMessage::addCallback()

MSceneMessage::addCheckCallback()

In the callbacks functions, just print out “The callback registered for MSceneMessage::kXXXX is executed.” Also in the callback function for MSceneMessage::kBeforeSaveCheck, set “retCode” to be pointing to “false” to abort current operation.

In undoIt() function, remove callbacks.

In doIt() function, call redoIt().

* + 4. In sceneMsgCmd, implement both initializePlugin() and uninitializePlugin() functions to handle registration and de-registration of the sceneMsgCmd command.

Relevant classes and methods:

MFnPlugin::registerCommand()

MFnPlugin::deregisterCommand()

Note: In uninitializePlugin() , don’t forget to remove all the callbacks you have registered in your plug-in.

* **Result**

After you finish and load the plug-in sceneMsgCmd.py, execute the follow command:

sceneMsgCmd;

When you open a file, there will be a print out in the output window:

“The callback registered for MSceneMessage::kBeforeOpen is executed.”

After you create a new file, there will be a print out in the output window:

“The callback registered for MSceneMessage::kAfterNew is executed.”

When you try to save current scene file, there will be a print out in the output window:

"The callback registered for MSceneMessage::kBeforeSaveCheck is executed."

There is also an error message popping up in Maya saying “File operation cancelled by user supplied callback” and the file is not saved.

**Assignment #7**

Manipulators

**arrowLocatorManip Plug-in**

* **Topics Covered**

Implement a custom manipulator with MPxManipContainer and MFnDiscManip. It manipulates the attribute “windDirection” on an arrowLocator node, which is implemented as custom locator from last asssignment. This Plug-in demonstrates how to set up affecting relationship between base manipulators and plugs on nodes.

* **Overview**

In this Plug-in, we will create a custom manipulator called “arrowLocatorManip”, user can use this manipulator to change the value of the “windDirection” attribute on a arrowLocator node.

* **Exercises**
  + 1. Double click on arrowLocatorManip.py, the skeleton of the arrowLocatorManip has already been provided.
  + 2. In arrowLocatorManip.py, register your custom manipulator

Relevant classes and methods:  
MFnPlugin::registerNode()

Please note that the name of your manipulator has to follow the name of your locator, otherwise Maya will not know how to connect them.

* + 3. Double click on arrowLocatorManip.py, go into arrowLocator::initialize() function, add one line to make connection between your custom node and your custom manipulator

Relevant classes and methods:

MPxManipContainer::addToManipConnectTable()

* + 4. Implement arrowLocatorManip.py, in arrowLocatorManip::createChildren() , create a base disc manip and add it into this manip container,

In arrowLocatorManip::connectToDependNode(), connect the "windDirection" plug on the locator node with the disc manip

Relevant classes and methods:

MPxManipContainer:: addDiscManip()

MFnDiscManip::connectToAnglePlug()

* **Result**

Load the arrowLocatorManip.py in Maya, in script editor, execute:

createNode arrowLocator,

the arrow locator is created in Maya viewport, then click on the “Show Manipulator Tool” on the toolbar, you will see a disc manip created at the center of the locator, rotating the disc manip will be changing the value of “windDirection” and the arrow locator will be rotating correspondingly.

* **Bonus section**

In this example, if you move your locator in Maya viewport and then show the manipulator, the manipulator stays at the original location. But if you uncomment the code in connectToDependNode() where it registers a plug to manip conversion callback , and also uncomment the callback function, and build the code and load in Maya again, you will see whenever the locator moves, the center position of the manipulator moves with it. You can remove the callback function code and try to implement it by yourself.